{"text_format":"1","workbook":"xlsx","n_sheets":7,"sheets":["Rückwärtsrechnung","Rückwärtsrechnung 2 Varianten","Rückwärtsrechnung Zeit","Vorwärtsrechnung 2 Varianten","Vorwärtsrechnung","Vorwärtsrechnung Weg","Beschleunigung 2 Varianten"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Rückwärtsrechnung","index":0,"n_rows":15,"n_cols":3,"rows_kept":15,"cut":false,"hidden":false,"merged":[[0,0,0,2]]}
["Rückwärtsrechnung\nAnalysebedingungen / Ergebnisse"]
["Mittlere Bremsverzögerung","m/s²",8]
["Vollbremsstrecke","m",12]
["Bremsschwellstrecke","m",{"$f":"(C8+C9)/3.6*C11/2","v":2.8512812921102033}]
["Reaktionsstrecke","m",{"$f":"C9/3.6*C12","v":11.725125168440815}]
["Reaktionspunkt (räumlich)","m",{"$f":"SUM(C3:C5)","v":26.57640646055102}]
["Anfangsgeschwindigkeit","km/h",0]
["Vollbremsgeschwindigkeit","km/h",{"$f":"(SQRT(C7/3.6*C7/3.6+2*C2*C3))*3.6","v":49.883063257983665}]
["Bremsausgangsgeschwindigkeit","km/h",{"$f":"(C8/3.6+C2/2*C11)*3.6","v":52.763063257983667}]
["Vollbremsdauer","s",{"$f":"(C8-C7)/3.6/C2","v":1.7320508075688772}]
["Bremsschwelldauer","s",0.2]
["Reaktionsdauer","s",0.8]
["Reaktionspunkt (zeitlich)","s",{"$f":"SUM(C10:C12)","v":2.7320508075688772}]
[]
["Berechnungsanlage "]

{"sheet":"Rückwärtsrechnung 2 Varianten","index":1,"n_rows":15,"n_cols":4,"rows_kept":15,"cut":false,"hidden":false,"merged":[[0,0,0,2]]}
["Rückwärtsrechnung\nAnalysebedingungen / Ergebnisse"]
["Mittlere Bremsverzögerung","m/s²",8,8.5]
["Vollbremsstrecke","m",32,{"$f":"C3","v":32}]
["Bremsschwellstrecke","m",{"$f":"(C8+C9)/3.6*C11/2","v":4.6054833995939042},{"$f":"(D8+D9)/3.6*D11/2","v":4.7497615158762407}]
["Reaktionsstrecke","m",{"$f":"C9/3.6*C12","v":18.741933598375621},{"$f":"D9/3.6*D12","v":19.339046063504966}]
["Reaktionspunkt (räumlich)","m",{"$f":"SUM(C3:C5)","v":55.347416997969532},{"$f":"SUM(D3:D5)","v":56.088807579381211}]
["Anfangsgeschwindigkeit","km/h",0,0]
["Vollbremsgeschwindigkeit","km/h",{"$f":"(SQRT(C7/3.6*C7/3.6+2*C2*C3))*3.6","v":81.458701192690285},{"$f":"(SQRT(D7/3.6*D7/3.6+2*D2*D3))*3.6","v":83.965707285772339}]
["Bremsausgangsgeschwindigkeit","km/h",{"$f":"(C8/3.6+C2/2*C11)*3.6","v":84.33870119269028},{"$f":"(D8/3.6+D2/2*D11)*3.6","v":87.025707285772356}]
["Vollbremsdauer","s",{"$f":"(C8-C7)/3.6/C2","v":2.8284271247461903},{"$f":"(D8-D7)/3.6/D2","v":2.743977362280142}]
["Bremsschwelldauer","s",0.2,{"$f":"C11","v":0.2}]
["Reaktionsdauer","s",0.8,{"$f":"C12","v":0.8}]
["Reaktionspunkt (zeitlich)","s",{"$f":"SUM(C10:C12)","v":3.8284271247461907},{"$f":"SUM(D10:D12)","v":3.743977362280142}]
[]
["Berechnungsanlage "]

{"sheet":"Rückwärtsrechnung Zeit","index":2,"n_rows":15,"n_cols":3,"rows_kept":15,"cut":false,"hidden":false,"merged":[[0,0,0,2]]}
["Rückwärtsrechnung\nAnalysebedingungen / Ergebnisse"]
["Mittlere Bremsverzögerung","m/s²",8]
["Vollbremsstrecke","m",{"$f":"(C8/3.6*C8/3.6-C7/3.6*C7/3.6)/2/C2","v":36.000000000000007}]
["Bremsschwellstrecke","m",{"$f":"(C8+C9)/3.6*C11/2","v":4.88}]
["Reaktionsstrecke","m",{"$f":"C9/3.6*C12","v":19.840000000000003}]
["Reaktionspunkt (räumlich)","m",{"$f":"SUM(C3:C5)","v":60.720000000000013}]
["Anfangsgeschwindigkeit","km/h",0]
["Vollbremsgeschwindigkeit","km/h",{"$f":"(C7/3.6+C2*C10)*3.6","v":86.4}]
["Bremsausgangsgeschwindigkeit","km/h",{"$f":"(C8/3.6+C2/2*C11)*3.6","v":89.28}]
["Vollbremsdauer","s",3]
["Bremsschwelldauer","s",0.2]
["Reaktionsdauer","s",0.8]
["Reaktionspunkt (zeitlich)","s",{"$f":"SUM(C10:C12)","v":4}]
[]
["Berechnungsanlage "]

{"sheet":"Vorwärtsrechnung 2 Varianten","index":3,"n_rows":15,"n_cols":4,"rows_kept":15,"cut":false,"hidden":false,"merged":[[0,0,0,2]]}
["Vorwärtsrechnung\nAnalysebedingungen / Ergebnisse"]
["Mittlere Bremsverzögerung","m/s²",3,4]
["Vollbremsstrecke","m",{"$f":"(C8/3.6*C8/3.6-C7/3.6*C7/3.6)/2/C2","v":19.480020576131682},{"$f":"(D8/3.6*D8/3.6-D7/3.6*D7/3.6)/2/D2","v":22.743765432098765}]
["Bremsschwellstrecke","m",{"$f":"(C8+C9)/3.6*C11/2","v":2.1922222222222216},{"$f":"(D8+D9)/3.6*D11/2","v":2.7377777777777776}]
["Reaktionsstrecke","m",{"$f":"C9/3.6*C12","v":8.8888888888888893},{"$f":"D9/3.6*D12","v":11.111111111111112}]
["Reaktionspunkt (räumlich)","m",{"$f":"SUM(C3:C5)","v":30.561131687242792},{"$f":"SUM(D3:D5)","v":36.592654320987656}]
["Endgeschwindigkeit","km/h",0,{"$f":"$C7","v":0}]
["Vollbremsgeschwindigkeit","km/h",{"$f":"(C9/3.6-C2/2*C11)*3.6","v":38.919999999999995},{"$f":"(D9/3.6-D2/2*D11)*3.6","v":48.56}]
["Bremsausgangsgeschwindigkeit","km/h",40,50]
["Vollbremsdauer","s",{"$f":"(C8-C7)/3.6/C2","v":3.6037037037037032},{"$f":"(D8-D7)/3.6/D2","v":3.3722222222222222}]
["Bremsschwelldauer","s",0.2,{"$f":"$C11","v":0.2}]
["Reaktionsdauer","s",0.8,{"$f":"$C12","v":0.8}]
["Reaktionspunkt (zeitlich)","s",{"$f":"SUM(C10:C12)","v":4.6037037037037036},{"$f":"SUM(D10:D12)","v":4.3722222222222227}]
[]
["Berechnungsanlage "]

{"sheet":"Vorwärtsrechnung","index":4,"n_rows":15,"n_cols":3,"rows_kept":15,"cut":false,"hidden":false,"merged":[[0,0,0,2]]}
["Vorwärtsrechnung\nAnalysebedingungen / Ergebnisse"]
["Mittlere Bremsverzögerung","m/s²",8]
["Vollbremsstrecke","m",{"$f":"(C8/3.6*C8/3.6-C7/3.6*C7/3.6)/2/C2","v":10.707438271604937}]
["Bremsschwellstrecke","m",{"$f":"(C8+C9)/3.6*C11/2","v":2.6977777777777781}]
["Reaktionsstrecke","m",{"$f":"C9/3.6*C12","v":11.111111111111112}]
["Reaktionspunkt (räumlich)","m",{"$f":"SUM(C3:C5)","v":24.51632716049383}]
["Endgeschwindigkeit","km/h",0]
["Vollbremsgeschwindigkeit","km/h",{"$f":"(C9/3.6-C2/2*C11)*3.6","v":47.12}]
["Bremsausgangsgeschwindigkeit","km/h",50]
["Vollbremsdauer","s",{"$f":"(C8-C7)/3.6/C2","v":1.6361111111111111}]
["Bremsschwelldauer","s",0.2]
["Reaktionsdauer","s",0.8]
["Reaktionspunkt (zeitlich)","s",{"$f":"SUM(C10:C12)","v":2.6361111111111111}]
[]
["Berechnungsanlage "]

{"sheet":"Vorwärtsrechnung Weg","index":5,"n_rows":15,"n_cols":3,"rows_kept":15,"cut":false,"hidden":false,"merged":[[0,0,0,2]]}
["Vorwärtsrechnung\nAnalysebedingungen / Ergebnisse"]
["Mittlere Bremsverzögerung","m/s²",8]
["Vollbremsstrecke","m",15]
["Bremsschwellstrecke","m",{"$f":"(C8+C9)/3.6*C11/2","v":3.2533333333333334}]
["Reaktionsstrecke","m",{"$f":"C9/3.6*C12","v":13.333333333333336}]
["Reaktionspunkt (räumlich)","m",{"$f":"SUM(C3:C5)","v":31.58666666666667}]
["Endgeschwindigkeit","km/h",{"$f":"3.6*SQRT(C8/3.6*C8/3.6-2*C2*C3)","v":12.340761726895153}]
["Vollbremsgeschwindigkeit","km/h",{"$f":"(C9/3.6-C2/2*C11)*3.6","v":57.120000000000005}]
["Bremsausgangsgeschwindigkeit","km/h",60]
["Vollbremsdauer","s",{"$f":"(C8-C7)/3.6/C2","v":1.5548346622605851}]
["Bremsschwelldauer","s",0.2]
["Reaktionsdauer","s",0.8]
["Reaktionspunkt (zeitlich)","s",{"$f":"SUM(C10:C12)","v":2.5548346622605851}]
[]
["Berechnungsanlage "]

{"sheet":"Beschleunigung 2 Varianten","index":6,"n_rows":8,"n_cols":4,"rows_kept":8,"cut":false,"hidden":false,"merged":[[0,0,0,2]]}
["Beschleunigung\nAnalysebedingungen / Ergebnisse"]
["Mittlere Beschleunigung","m/s²",1,1]
["Beschleunigungsstrecke","m",{"$f":"(C5/3.6*C5/3.6-C4/3.6*C4/3.6)/2/C2","v":8.6805555555555571},{"$f":"(D5/3.6*D5/3.6-D4/3.6*D4/3.6)/2/D2","v":15.432098765432098}]
["Anfangsgeschwindigkeit","km/h",0,{"$f":"$C4","v":0}]
["Endgeschwindigkeit","km/h",15,20]
["Beschleunigungsdauer","s",{"$f":"(C5-C4)/3.6/C2","v":4.166666666666667},{"$f":"(D5-D4)/3.6/D2","v":5.5555555555555554}]
[]
["Berechnungsanlage 1"]